**Problem 2-10:** A coordinate measuring machine has sampled the slot feature surfaces and has generated the 3D pattern of points shown below. The gage is 3D. Based on this data, does this slot pass the m modified flatness tolerance?

19.5 mm GO Gage – 3D

Slot surfaces – 3D