**Problem 4-2:** A coordinate measuring machine has sampled a rail feature surfaces and has generated the 3D pattern of points shown below. The gage is 3D. Based on this data, does this rail pass the MMC modified perpendicularity tolerance?



21.2 mm GO Gage – 3D

Rail surface

Datum A surface 3D