**Problem 4-3:** A coordinate measuring machine has sampled a hole feature surface and has generated the 3D pattern of points shown below. The gage is 3D. Based on this data, does this rail pass the MMC modified perpendicularity tolerance?



21 mm GO Gage – 3D

Hole surface

Datum A surface 3D