**Problem 4-5:** A coordinate measuring machine has sampled a hole feature surface and has generated the 3D pattern of points shown below.



Moving the drawing below the points, show the size of the OCAME as indicated by the green lines (the distance between the green lines is OCAME). The center line is the axis of the OCAME.

Hole surface

Datum A surface 3D